**Syringe pumps**

* Programmable drug protocols
* Dose calculation based on dosages, patient weight and time
* Bolus function
* It may works with different types and brands of syringes
* 12 V low voltage power supply with external transformer
* Rechargeable battery with an autonomy of approximately 8h at 25 ml/h
* electronic state of charge and cycler (automatic)
* Large and bright display for easy reading of all parameters and any alarms
* Alarms
* Stackable
* Rack
* preferably compliant with the Italian medical devices legislation in force in Italy applied to medical devices.
* Supply: 220 V, 50 Hz
* IEC 60601-1 class;
* protected against dripping IP 22